

**Current system taking roof water from 2 and 4 Erw Las. Outlet is currently unknown. Proposed that we connect into the new drainage system.**

**Proposed two new manholes and 9” pipe, allowing surface water to discharge upstream of the bridge at Erw Las.**

**Current surface water drainage system.**

